2013-08-01 Post Flight performed by Jon Gero
2013-08-02 all times UTC

Timeline:
	•	Connect Artoo to SHIS under DSC battery power
	•	1511 ON
	•	1511 ping OK
	•	1511 start data transfer from S-HIS DSC to Artoo	
	⁃	sh130801
	•	 telnet in to S-HIS
	•	 checked diskspace on DSC, 14% used
	•	 created MD5SUM
	•	1516 finished data transfer of sh130801 files and md5sum
	•	1516 DSC OFF
	•	Inspected mirror, no need for cleaning -or- cleaned mirror if required
	•	Mirror manually set to pre-flight position (orange line down)

	•	Connect Artoo to GH aircraft network, set Artoo location to GlobalHawk
	•	1721 request DC41, DC42, IL41 (sounding) ON
	•	1721 ping OK
	•	1721 run dashboard, verified S-HIS operating nominally, 
	•	1724 visible verification of scene mirror rotation
	•	Run instrument for 15 mins
	•	1733 detector temp < 80K (green status light)
	•	1734 detector temp stable @ 76K
	•	1736 IL42 (descent heaters) ON, verified BB temp change, bus 2 current, and DA Voltage change
	•	1736 IL42 OFF
	•	1737 start data transfer from S-HIS DSC to PHASE	
	⁃	sh130802
	•	1737 telnet in to S-HIS
	•	1738 killed data collect, highest temperature was DSC PCI temp @ 320K (all green lights)
	•	1738 cleared disk space, now at 5%, removed
	⁃	sh130801
	•	1738 created MD5SUM
	•	1738 finished data transfer of sh130802 files and md5sum
	•	1740 IL41, DC41, DC42 OFF
	•	Inspected mirror, no need for cleaning -or- cleaned mirror if required
	•	Mirror manually set to pre-flight position (orange line down)

Notes:
	•	First downloaded data under battery power
	•	A/C power was available later in the day for post-flight
	•	Engineering data looks nominal

Commands and their output:

######################################################################
Terminal #1A:
######################################################################

Last login: Thu Aug  1 19:26:17 on ttys000
qwaihir-130134160014: ping 10.3.1.130PING 10.3.1.130 (10.3.1.130): 56 data bytes
64 bytes from 10.3.1.130: icmp_seq=0 ttl=64 time=0.452 ms
64 bytes from 10.3.1.130: icmp_seq=1 ttl=64 time=0.545 ms
64 bytes from 10.3.1.130: icmp_seq=2 ttl=64 time=0.428 ms
^C
--- 10.3.1.130 ping statistics ---
3 packets transmitted, 3 packets received, 0.0% packet loss
round-trip min/avg/max/stddev = 0.428/0.475/0.545/0.050 ms
qwaihir-130134160014: rsync -uav --progress rsync://10.3.1.130/data/sh130801 ~/RAW_DATA/.
receiving file list ... 
15 files to consider
sh130801/
sh130801/SOH.log
        1458 100%    1.39MB/s    0:00:00 (xfer#1, to-check=13/15)
sh130801/eltsmbz.rsh
   167692492 100%    8.32MB/s    0:00:19 (xfer#2, to-check=12/15)
sh130801/eltsotg.rsh
   163430616 100%    8.83MB/s    0:00:17 (xfer#3, to-check=11/15)
sh130801/eltsrkn.rsh
   167939664 100%    8.12MB/s    0:00:19 (xfer#4, to-check=10/15)
sh130801/eltsubu.rsh
   169628112 100%    8.63MB/s    0:00:18 (xfer#5, to-check=9/15)
sh130801/eltswtb.rsh
   171683528 100%    8.23MB/s    0:00:19 (xfer#6, to-check=8/15)
sh130801/eltszki.rsh
   173527252 100%    8.50MB/s    0:00:19 (xfer#7, to-check=7/15)
sh130801/elttcbp.rsh
   175278496 100%    8.32MB/s    0:00:20 (xfer#8, to-check=6/15)
sh130801/elttesw.rsh
   176700628 100%    8.84MB/s    0:00:19 (xfer#9, to-check=5/15)
sh130801/eltthkd.rsh
   179621524 100%    8.47MB/s    0:00:20 (xfer#10, to-check=4/15)
sh130801/elttkbk.rsh
    91485872 100%    8.63MB/s    0:00:10 (xfer#11, to-check=3/15)
sh130801/shisam_130801_135514.log1
           0 100%    0.00kB/s    0:00:00 (xfer#12, to-check=2/15)
sh130801/shisam_130801_135514.log2
     9126701 100%    7.43MB/s    0:00:01 (xfer#13, to-check=1/15)
sh130801/timestamp.out
      142785 100%  753.72kB/s    0:00:00 (xfer#14, to-check=0/15)

sent 395 bytes  received 1646461082 bytes  9021706.72 bytes/sec
total size is 1646259128  speedup is 1.00
qwaihir-130134160014: rsync -uav --progress rsync://10.3.1.130/data/sh130801 ~/RAW_DATA/.
receiving file list ... 
16 files to consider
sh130801/
sh130801/MD5SUM
         460 100%  449.22kB/s    0:00:00 (xfer#1, to-check=14/16)

sent 109 bytes  received 901 bytes  2020.00 bytes/sec
total size is 1646259588  speedup is 1629959.99
qwaihir-130134160014: cd ~/RAW_DATA/sh130801
qwaihir-130134160014: md5sum -cv MD5SUM
eltsmbz.rsh    OK
eltsotg.rsh    OK
eltsrkn.rsh    OK
eltsubu.rsh    OK
eltswtb.rsh    OK
eltszki.rsh    OK
elttcbp.rsh    OK
elttesw.rsh    OK
eltthkd.rsh    OK
elttkbk.rsh    OK
qwaihir-130134160014:

######################################################################
Terminal #2A:
######################################################################

Last login: Thu Aug  1 17:52:00 on ttys000
qwaihir-130134160014: telnet -l root 10.3.1.130
Trying 10.3.1.130...
Connected to shis.
Escape character is '^]'.
Linux myrouter 2.4.26 #6 Tue Jun 15 16:59:15 GMT 2004 i386 unknown

Type in help if you are really lost

myrouter# df
Filesystem           1k-blocks      Used Available Use% Mounted on
/dev/ram0                16208      8528      7680  53% /
/dev/hda2             16575544   2267648  14307896  14% /data
myrouter# cd /data
myrouter# ls
SOH            bin            lib            man            opt
tmp            Backup         soh_pipe       MD5SUM         motor
scripts        rc.local.gh    sh130801       sh130802       rc.local.bak
rc.local.er2   rc.local.bak2  Software       include        rc.local
myrouter# ls -l
drwxr-xr-x    2 root     root         920 Jul 28  2007 SOH
drwxr-xr-x    2 root     root         240 Jul 12  2007 bin
drwxr-xr-x    3 root     root         272 Jul 12  2007 lib
drwxr-xr-x    3 root     root          72 Jul 12  2007 man
drwxr-xr-x    6 root     root         144 Jul  6  2007 opt
drwxr-xr-x    4 root     root         184 Aug  2  2012 tmp
drwxr-xr-x    3 root     root         144 Jun 19  2007 Backup
-rw-r--r--    1 root     root        1205 Jul  7  2007 soh_pipe
-rw-r--r--    1 root     root           0 Aug 31  2011 MD5SUM
drwxr-xr-x    2 root     root         912 Oct 28  2011 motor
drwxr-xr-x    2 root     root          80 Jun 19  2007 scripts
-rwx--x--x    1 root     root         579 Jul 15 22:11 rc.local.gh
drwxr-xr-x    2 root     root         520 Aug  1 18:25 sh130801
drwxr-xr-x    2 root     root         168 Aug  2 15:11 sh130802
-rwx--x--x    1 root     root         579 Apr 25 16:20 rc.local.bak
-rwx--x--x    1 root     root         580 Jul 15 22:11 rc.local.er2
-rwx--x--x    1 root     root         580 May 17 16:27 rc.local.bak2
drwxr-xr-x    5 root     root        2880 Sep 23  2012 Software
drwxr-xr-x    3 root     root          80 Jul 12  2007 include
-rwx--x--x    1 root     root         828 Jul 16 15:51 rc.local
myrouter# cd /data/sh130801
myrouter# ls
eltsrkn.rsh                SOH.log                    eltthkd.rsh
eltszki.rsh                shisam_130801_135514.log1  shisam_130801_135514.log2
eltsmbz.rsh                elttcbp.rsh                eltsubu.rsh
elttkbk.rsh                timestamp.out              eltsotg.rsh
elttesw.rsh                eltswtb.rsh
myrouter# ls -l *.rsh
-rw-r--r--    1 root     root    167692492 Aug  1 14:25 eltsmbz.rsh
-rw-r--r--    1 root     root    163430616 Aug  1 14:55 eltsotg.rsh
-rw-r--r--    1 root     root    167939664 Aug  1 15:25 eltsrkn.rsh
-rw-r--r--    1 root     root    169628112 Aug  1 15:55 eltsubu.rsh
-rw-r--r--    1 root     root    171683528 Aug  1 16:25 eltswtb.rsh
-rw-r--r--    1 root     root    173527252 Aug  1 16:55 eltszki.rsh
-rw-r--r--    1 root     root    175278496 Aug  1 17:25 elttcbp.rsh
-rw-r--r--    1 root     root    176700628 Aug  1 17:55 elttesw.rsh
-rw-r--r--    1 root     root    179621524 Aug  1 18:25 eltthkd.rsh
-rw-r--r--    1 root     root    91485872 Aug  1 18:40 elttkbk.rsh
myrouter# cd /data/sh130802
myrouter# ls
SOH.log                    shisam_130802_151119.log1  shisam_130802_151119.log2
myrouter# ls -l *.rsh
*.rsh: No such file or directory
myrouter# cd /data/sh130801
myrouter# /data/Software/md5sum *.rsh > MD5SUM
myrouter# 

######################################################################
Terminal #1B:
######################################################################

Last login: Fri Aug  2 16:00:16 on ttys000
qwaihir-130134160014: ping 10.3.1.130
PING 10.3.1.130 (10.3.1.130): 56 data bytes
64 bytes from 10.3.1.130: icmp_seq=0 ttl=64 time=1.019 ms
64 bytes from 10.3.1.130: icmp_seq=1 ttl=64 time=0.598 ms
64 bytes from 10.3.1.130: icmp_seq=2 ttl=64 time=0.600 ms
^C
--- 10.3.1.130 ping statistics ---
3 packets transmitted, 3 packets received, 0.0% packet loss
round-trip min/avg/max/stddev = 0.598/0.739/1.019/0.198 ms
qwaihir-130134160014: rsync -uav --progress rsync://10.3.1.130/data/sh130802 ~/RAW_DATA/.
receiving file list ... 
8 files to consider
sh130802/
sh130802/SOH.log
        2916 100%    2.78MB/s    0:00:00 (xfer#1, to-check=6/8)
sh130802/eltyceb.rsh
    92342712 100%    5.52MB/s    0:00:15 (xfer#2, to-check=5/8)
sh130802/shisam_130802_151119.log1
           0 100%    0.00kB/s    0:00:00 (xfer#3, to-check=4/8)
sh130802/shisam_130802_151119.log2
         622 100%    0.98kB/s    0:00:00 (xfer#4, to-check=3/8)
sh130802/shisam_130802_172104.log1
           0 100%    0.00kB/s    0:00:00 (xfer#5, to-check=2/8)
sh130802/shisam_130802_172104.log2
      520254 100%  767.46kB/s    0:00:00 (xfer#6, to-check=1/8)
sh130802/timestamp.out
        9341 100%   13.76kB/s    0:00:00 (xfer#7, to-check=0/8)

sent 241 bytes  received 92896394 bytes  5630099.09 bytes/sec
total size is 92875845  speedup is 1.00
qwaihir-130134160014: rsync -uav --progress rsync://10.3.1.130/data/sh130802 ~/RAW_DATA/.
receiving file list ... 
9 files to consider
sh130802/
sh130802/MD5SUM
          46 100%   44.92kB/s    0:00:00 (xfer#1, to-check=7/9)
sh130802/eltyceb.rsh
    95893676 100%    8.86MB/s    0:00:10 (xfer#2, to-check=5/9)
sh130802/shisam_130802_172104.log2
      541335 100%  812.05kB/s    0:00:00 (xfer#3, to-check=1/9)

sent 71847 bytes  received 3606294 bytes  319838.35 bytes/sec
total size is 96447936  speedup is 26.22
qwaihir-130134160014: cd ~/RAW_DATA/sh130802
qwaihir-130134160014: md5sum -cv MD5SUM
eltyceb.rsh    OK
qwaihir-130134160014: 

######################################################################
Terminal #2B:
######################################################################

Last login: Fri Aug  2 15:46:36 on ttys000
qwaihir-130134160014: telnet -l root 10.3.1.130
Trying 10.3.1.130...
Connected to shis.
Escape character is '^]'.
Linux myrouter 2.4.26 #6 Tue Jun 15 16:59:15 GMT 2004 i386 unknown

Type in help if you are really lost

myrouter# rm -rf /data/sh130801
myrouter# df
Filesystem           1k-blocks      Used Available Use% Mounted on
/dev/ram0                16208      8533      7675  53% /
/dev/hda2             16575544    751312  15824232   5% /data
myrouter# echo hi > /tmp/operator 
myrouter# killall -9 shisam
myrouter# cd /data/sh130802
myrouter# ls
SOH.log                    shisam_130802_172104.log1  shisam_130802_172104.log2
eltyceb.rsh                shisam_130802_151119.log1  shisam_130802_151119.log2
timestamp.out
myrouter# ls -l *.rsh
-rw-r--r--    1 root     root    95893676 Aug  2 17:38 eltyceb.rsh
myrouter# /data/Software/md5sum *.rsh > MD5SUM
myrouter#